| Actimux DCU : Error frame #1 description This signal is transmitted from DCU to the vehicle within the message DCU_Veh_#1, a mask is applied to the value to extract information:

Signal value | Mnemonic | Description
0000 0000 | --- | No active error.
xxxx xxx1 | Fault1 | Open load detected for at least 1 sensitive edge.
xxxx xx1x | Fault2 | Buzzer short circuit detected.
xxxx x1xx | Fault3 | Entrance lights short circuit detected.
xxxx 1xxx | Fault4 | Not used.
xxx1 xxxx | Fault5 | Electric motor open load detected.
xx1x xxxx | Fault6 | Electric motor short circuit detected.
x1xx xxxx | Fault7 | Electric motor-brake open load detected.
1xxx xxxx | Fault8 | Electric motor-brake short circuit detected.

Copyright © ACTIA 2015