ActiGRAF Help : MASTER25 LS1A output Description

##### 1 - Parameters Description

##### 2 - Mnemonics Description

The mnemonics names for ECU IO must applies a set of rules more details.

Mnemonic | STraToN Type | Description
--- | --- | ---
Output_Boo | BOOL | boolean command of the output.
Fault | BOOL | indicates if a fault is detected on the output.
Fault_Type | BOOL | indicate the type of fault : 0 for SC fault and 1 for OC fault.
Equipment | BOOL | To manage the Fault detection ( more details ).

Copyright © ACTIA 2013