Label		Connection		DataType		IsInput		Address		ImportField		MMI_Order		Description		
Speed/standstill signal		Output_Boo		BOO		False		0B0C60				6		Power_OutBoo_Conn		
Reset/inhibit emergency valve		Output_Boo		BOO		False		0B0C61				6		Power_OutBoo_Conn		
Passenger halt release indicator		Output_Boo		BOO		False		0B0C62				6		Power_OutBoo_Conn		
Wheelchair halt release indicator		Output_Boo		BOO		False		0B0C63				6		Power_OutBoo_Conn		
Door request		Output_Ana		ANA		False		0B0C40				6		OUT_ANA_CMD		
Door position request left/both leaf(s)		Output_Ana		ANA		False		0B0C42				6		OUT_ANA_CMD		
Door position request right leaf		Output_Ana		ANA		False		0B0C44				6		OUT_ANA_CMD		
Disable Obstruction Security's		Output_Ana		ANA		False		0B0C46				6		OUT_ANA_CMD		
Spare out 1 request		Output_Boo		BOO		False		0B0C5A						Power_OutBoo_Conn		
Spare out 2 request		Output_Boo		BOO		False		0B0C5B						Power_OutBoo_Conn		
Spare out 3 request		Output_Boo		BOO		False		0B0C5C						Power_OutBoo_Conn		
Spare out 4 request		Output_Boo		BOO		False		0B0C5D						Power_OutBoo_Conn		
Spare out 5 request		Output_Boo		BOO		False		0B0C5E						Power_OutBoo_Conn		
Spare out 6 request		Output_Boo		BOO		False		0B0C5F						Power_OutBoo_Conn		
Entrance Lights Request		Output_Boo		BOO		False		0B0C64				6		Power_OutBoo_Conn		
Buzzer Request		Output_Boo		BOO		False		0B0C66				6		Power_OutBoo_Conn		
Door system type 0		Input_Boo		BOO		True		0B0C26						LCC_DescConn15		
Door system type 1		Input_Boo		BOO		True		0B0BE7						LCC_DescConn15		
Door system type 2		Input_Boo		BOO		True		0B0C03						LCC_DescConn15		
Door system type 3		Input_Boo		BOO		True		0B0C04						LCC_DescConn15		
Door system type 4		Input_Boo		BOO		True		0B0C07						LCC_DescConn15		
Door system type 5		Input_Boo		BOO		True		0B0C08						LCC_DescConn15		
Door system type 6		Input_Boo		BOO		True		0B0C09						LCC_DescConn15		
Door system type 7		Input_Boo		BOO		True		0B0C0A						LCC_DescConn15		
Spare in 1 status		Input_Boo		BOO		True		0B0BE8						LCC_DescConn15		
Spare in 2 status		Input_Boo		BOO		True		0B0BE9						LCC_DescConn15		
Spare in 3 status		Input_Boo		BOO		True		0B0BEA						LCC_DescConn15		
Spare in 4 status		Input_Boo		BOO		True		0B0BEB						LCC_DescConn15		
Workshop button		Input_Boo		BOO		True		0B0C0D				6		LCC_DescConn15		
External open button		Input_Boo		BOO		True		0B0C0E				6		LCC_DescConn15		
External close button		Input_Boo		BOO		True		0B0C0F				6		LCC_DescConn15		
Passenger halt request button		Input_Boo		BOO		True		0B0C10				6		LCC_DescConn15		
Wheelchair halt request		Input_Boo		BOO		True		0B0C11				6		LCC_DescConn15		
Sensitive edge inner input status		Input_Boo		BOO		True		0B0C05				6		LCC_DescConn15		
Sensitive edge outer input status		Input_Boo		BOO		True		0B0C06				6		LCC_DescConn15		
Light Barrier #1 input status		Input_Boo		BOO		True		0B0BEE				6		LCC_DescConn15		
Light Barrier #2 input status		Input_Boo		BOO		True		0B0BEF				6		LCC_DescConn15		
End Switch input status		Input_Boo		BOO		True		0B0BF0				6		LCC_DescConn15		
Emergency pressure switch input status		Input_Boo		BOO		True		0B0BF1				1		LCC_DescConn15		
Emergency pressure switch input 2 status		Input_Boo		BOO		True		0B0C0B				1		LCC_DescConn15		
Open load detected for at least 1 sensitive edge		Input_Boo		BOO		True		0B0BFB				1		LCC_DescConn15		
Buzzer short circuit detected		Input_Boo		BOO		True		0B0BFC				2		LCC_DescConn15		
Entrance lights short circuit detected		Input_Boo		BOO		True		0B0C13				3		LCC_DescConn15		
//Not used		Input_Boo		BOO		True		0B0C14				4		LCC_DescConn15		
Electric motor open load detected (Left or both)		Input_Boo		BOO		True		0B0C15				5		LCC_DescConn15		
Electric motor short circuit detected (Left or both)		Input_Boo		BOO		True		0B0C16				6		LCC_DescConn15		
Electric motor-brake open load detected (Left or both)		Input_Boo		BOO		True		0B0C01				7		LCC_DescConn15		
Electric motor-brake short circuit detected (Left or both)		Input_Boo		BOO		True		0B0C02				8		LCC_DescConn15		
Power-supply Vbatt missing		Input_Boo		BOO		True		0B0BF2				1		LCC_DescConn15		
Power-supply V1 missing		Input_Boo		BOO		True		0B0BF3				2		LCC_DescConn15		
Position sensor power-supply short circuit detected		Input_Boo		BOO		True		0B0BF4				3		LCC_DescConn15		
Sensor power-supply short circuit detected		Input_Boo		BOO		True		0B0BF5				4		LCC_DescConn15		
Position input missing/invalid		Input_Boo		BOO		True		0B0BF6				5		LCC_DescConn15		
//Not used		Input_Boo		BOO		True		0B0BF7				6		LCC_DescConn15		
//Not used		Input_Boo		BOO		True		0B0BF8				7		LCC_DescConn15		
//Not used		Input_Boo		BOO		True		0B0BE6				8		LCC_DescConn15		
Open load detected for at least 1 sensitive edge (Right)		Input_Boo		BOO		True		0B0C1F				1		LCC_DescConn15		
//Not used		Input_Boo		BOO		True		0B0C20				1		LCC_DescConn15		
//Not used		Input_Boo		BOO		True		0B0C21				1		LCC_DescConn15		
//Not used		Input_Boo		BOO		True		0B0C22				1		LCC_DescConn15		
Electric motor open load detected (Right leaf)		Input_Boo		BOO		True		0B0C23				1		LCC_DescConn15		
Electric motor short circuit detected (Right leaf)		Input_Boo		BOO		True		0B0C24				1		LCC_DescConn15		
Electric motor-brake open load detected (Right leaf)		Input_Boo		BOO		True		0B0C25				1		LCC_DescConn15		
Electric motor-brake short circuit detected (Right leaf)		Input_Boo		BOO		True		0B0C1D				1		LCC_DescConn15		
VAMS input voltage		Input_Ana		ANA		True		0B0BBC				6		IN_ANA_STATUS		
V1 input voltage		Input_Ana		ANA		True		0B0BBE				6		IN_ANA_STATUS		
Vbatt input voltage		Input_Ana		ANA		True		0B0BC0				6		IN_ANA_STATUS		
Door position status left		Input_Ana		ANA		True		0B0B92				6		IN_ANA_STATUS		
Door Leaf status		Input_Ana		ANA		True		0B0B94				6		IN_ANA_STATUS		
Door Obstruction status		Input_Ana		ANA		True		0B0B96				6		IN_ANA_STATUS		
Door mode		Input_Ana		ANA		True		0B0B98				6		IN_ANA_STATUS		
Door position status right leaf		Input_Ana		ANA		True		0B0B9A				6		IN_ANA_STATUS		
Door position left/both leafs %		Input_Ana		ANA		True		0B0B9C				6		IN_ANA_STATUS		
Door position right leaf %		Input_Ana		ANA		True		0B0B9E				6		IN_ANA_STATUS		
Encoder pulse count		Input_Ana		ANA		True		0B0B90				6		IN_ANA_STATUS		
DCUDialogF		Input_Boo		BOO		True		0B0C77				1		IN_ANA_STATUS		
