| Actimux DCU : Door obstruction status description This signal is transmitted from DCU to the vehicle within the message DCU_Veh_#2:

Signal value | Description
0000 | No obstruction (Left or both).
0001 | Obstruction by sensitive edge open direction (Left or both).
0010 | Obstruction by sensitive edge close direction (Left or both).
0011 | Obstruction by light barrier #1 close direction (Left or both).
0100 | Obstruction by light barrier #2 close direction (Left or both).
0101 | Obstruction by door speed open direction (Left or both).
0110 | Obstruction by door speed close direction (Left or both).
0111 | Obstruction by Footstep (Left or both).
1000-1111 | Not used.
XXXX 0000 | No Obstruction (Right) (When applicable).
XXXX 0001 | Obstruction by sensitive edge open direction (Right).
XXXX 0010 | Obstruction by sensitive edge close direction (Right).
XXXX 0011 | Obstruction by light barrier #1 close direction (Right).
XXXX 0100 | Obstruction by light barrier #2 close direction (Right).
XXXX 0101 | Obstruction by door speed open direction (Right).
XXXX 0110 | Obstruction by door speed close direction (Right).
XXXX 0111 | Obstruction by Footstep (Right).
XXXX 1111 | Operation as separate doors not used.

Copyright © ACTIA 2015