ActiGRAF Help : MASTER25 Input Description
The configuration of the input on HS or LS is done by manufacturing parameter.

##### 1 - Parameters Description

Parameter | Description
--- | ---
Filter | define the filtering value for the logical input. the filter unit is Ms. When programming the ECU a resolution of 50 Ms is used, hence the increment unit is 50.

##### 2 - Mnemonics Description

The mnemonics names for ECU IO must applies a set of rules more details.

Mnemonic | Description
--- | ---
Input_Boo | Indicates the status of the input, the status evolution is shown in the following hysteresis where V1 and V2 are hradware defined thresholds:
- For HS configuration :
- For LS configuration :

Copyright © ACTIA 2012