| Actimux DCU : Door leaf status description This signal is transmitted from DCU to the vehicle within the message DCU_Veh_#2:

Signal value | Description
0000 | Door idle (Left or both).
0001 | Door opening (Left or both).
0010 | Door obstruction in open direction (Left or both).
0011 | Door obstruction idle (Left or both).
0100 | Door obstruction in close direction (Left or both).
0101 | Door closing (Left or both).
0110-1111 | Not used.
XXXX 0000 | Door idle (Right).
XXXX 0001 | Door opening (Right).
XXXX 0010 | Door obstruction in open direction (Right).
XXXX 0011 | Door obstruction idle (Right).
XXXX 0100 | Door obstruction in close direction (Right).
XXXX 0101 | Door closing (Right).
XXXX 0110-1111 1111 | Not used.

Copyright © ACTIA 2015