ActiGRAF Help : MASTER25 Sensor Supply output Description

This output provides a regulated voltage from 0 to 15 volts with respect to sensor supply command value received on the input CAN frame.

##### 1 - Parameters Description

Parameter | Description
--- | ---
Mode | To activate the output function as a :
- Not Used : output not used.
- Sensor Supply used : output used for a sensor supply function.
- Oil measurement used :output used for oil measurement function ( not available yet).

##### 2 - Mnemonics Description

Mnemonic | Description
--- | ---
Output_Ana | the voltage value to be applied on the Output. the value unit is mV. If the values is superior to 15 000 mV, the voltage on the output is limited to 15 000 mV.
Fault | If the difference between the CAN command and the voltage measured on the output is greater than 5%, then the Fault is set to 1.
Equipment | To manage the Fault detection ( more details ).

Copyright © ACTIA 2013