| Actimux DCU : Door system type description This signal is transmitted from DCU to the vehicle within the message DCU_Veh_#1. The signal value is calculated using boolean variables: door system type 0 to door system type 7 .

Signal value | Description
0001 XXXX | Rapid Slider (Left or both).
0010 XXXX | Plug Slider( Left or both).
0011 XXXX | Plug Slider 2 ( Left or both).
0100 XXXX | Outward Swinging (Left or both).
0101 XXXX | inward Gliding (Ventura doors) (Left or both).
0110 XXXX | inward Gliding (Iveco doors) (Left or both).
0111 XXXX-1111 XXXX | Not used.
XXXX 0000 | Door system not used (Right Leaf not as separate).
XXXX 0001 | Rapid Slider (Right Leaf as separate).
XXXX 0010 | Plug Slider (Right Leaf as separate).
XXXX 0011 | Plug Slider 2 (Right Leaf as separate).
XXXX 0100 | Outward Swinging (Right Leaf as separate).
XXXX 0101 | inward Gliding (Ventura doors) (Right Leaf as separate).
XXXX 0110 | inward Gliding (Iveco doors) (Right Leaf as separate).
XXXX 0111-XXXX 1111 | Not used.
0000 XXXX | illegal combination.

Copyright © ACTIA 2015