ActiGRAF Help : MASTER25 General Description

Parameter | Description
--- | ---
Deg Mode State Duration | define the duration of a state when the ECU is in degraded mode
Out CMD Per | define the period of the CMD frame. this parameter is not available for developer modification. Value's unit is 10 Ms
ECU Adr | to define the master ECU address:

Pin ADR | Logical Address | Address value
--- | --- | ---
Open circuit | 1 | D6H
GND | 2 | D9H
VBAT | 3 | DAH

Copyright © ACTIA 2012