ActiGRAF Help : MASTER25 Power Supply Description

Mnemonic | STraToN Type | Description
--- | --- | ---
VBAT_MEAS | WORD | input data about the VBAT measurement.
Fault | BOOL | TRUE : if VBAT is not present (VBAT < 12V). This case can happen when the vehicle batteries is very low the Power send this information just before his shut-down FALSE : if VBAT is present (VBAT > 12V) The variable name declared in STraToN dictionary must use the prefix "D_".

Copyright © ACTIA 2012