ActiGRAF Help : MASTER-DISPLAY CAN Description
CAN communication interfaces allow to connect other ECU and electronic components to the MASTER-DISPLAY calculator.
- The baud rate for each can be set. the baud rate value range is 0-1000 Kbaud. The baud value is fixed to 250 Kbaud if SwitchPack or Powers protocols is used.
- "User Protocol" can be used once on each CAN, so up to 5 instances in a wiring.
- On each CAN we can configure up to 3 different Protocols. A protocol can not be set twice in the same CAN or in different CANs (except "User Protocol").
- J1939A and J1939B can not be configured together in the same CAN.
- The first protocol of CAN 5, is always set to "SwitchPack" .
- "None" : means no protocol is used.
- "N/A" : indicates the use of undefined protocol.

Copyright © ACTIA 2015