| Actimux DCU : Error frame #2 description This signal is transmitted from DCU to the vehicle within the message DCU_Veh_#1, a mask is applied to the value to extract information:

Signal value | Mnemonic | Description
0000 0000 | --- | No active error.
xxxx xxx1 | Fault1 | Power-supply Vbatt missing.
xxxx xx1x | Fault2 | Power-supply V1 missing.
xxxx x1xx | Fault3 | Position sensor power-supply short circuit detected.
xxxx 1xxx | Fault4 | Sensor power-supply short circuit detected.
xxx1 xxxx | Fault5 | Position input missing/invalid.
xx1x xxxx | Fault6 | Not used.
x1xx xxxx | Fault7 | Not used.
1xxx xxxx | Fault8 | Not used.

Copyright © ACTIA 2015