ActiGRAF Help : MASTER25 HS2A output Description

##### 1-1 - Parameters Description

Category | parameter | Description
--- | --- | ---
General | Mode | Defines the Mode of use of the Output : static or dynamic.
Load Type | To set the type of load attached to the output : bulb load, Resistive load, Motion Motor load or FAN Motor Load.
Frequency range | To set the range of the frequency parameter, two range are available : High and low.
Frequency | To set the Frequency of the output, only in Dynamic mode.
Protection Profile | OC_Range | Defines output over-current range .
OC_NTHld | Defines output nominal threshold
OC_MTHld | Defines the output intermediate threshold. Only for output with a load of type BULB.
OC_HTHld | To set the output highest threshold.
OC_TIME | To set the output protection profile times(see protection profiles model below).
Bulb protection profile | This profile is applied when load type = "bulb load" or "Resistive load".
Motor protection profile | This profile is applied when load type = "Motion Motor load" or "FAN Motor Load".

##### 1-2 - Mnemonics Description

The mnemonics names for ECU IO must applies a set of rules more details.

Mnemonic | STraToN Type | Description
--- | --- | ---
Output_Dyn | WORD | The dynamic command of the output, sent only if dynamic Mode is set, value range is 0% to 100%
Output_Boo | BOOL | Boolean command of the output.
Current | WORD | value of current.
Fault | BOOL | indicates if a fault is detected on the output.
Fault_Type | BOOL | indicate the type of fault : 0 for SC fault and 1 for OC fault.
Equipment | BOOL | To manage the Fault detection ( more details ).

Copyright © ACTIA 2013