| Actimux DCU : Disable Obstruction Security's description This signal is transmitted from vehicle to DCU within the message Veh_DCU_#1, a mask is applied to the signal value to extract information:

Signal value | Description
0000 | No obstruction security's disabled.
xxx1 | Sensitive edge inner/left disabled.
xx1x | Sensitive edge outer/right disabled.
x1xx | Light Barrier #1 disabled.
1xxx | Light Barrier #2 disabled.

Copyright © ACTIA 2015