| Actimux DCU : Door request description This signal is transmitted from vehicle to DCU within the message Veh_DCU_#1:

Signal value | Description
0 | No request.
1 | Open request (Both leafs).
10 | Open request (left leaf).
11 | Open request (Rear leaf).
100 | Close request (Both leafs).
101 | Close request (Left leaf).
110 | Close request (Rear leaf).
111 | Stop request (Both leafs).
1000 | Stop request (Left leaf).
1001 | Stop request (Rear leaf).
1010 | Learn request (Both leafs).
1011 | Learn request (Left leaf).
1100 | Learn request (Rear leaf).

Copyright © ACTIA 2015