ActiGRAF Help : MASTER-DISPLAY Power Supply Description
The mnemonics names for ECU IO must applies a set of rules more details.

Fault | TRUE : if VBAT is not present (VBAT < 12V). This case can happen when the vehicle battery is very low the Power send this information just before his shut down FALSE : if VBAT is present (VBAT > 12V) This variable must use a specific naming see variable rules.

Copyright © ACTIA 2015