Gearshift viewer
|  | Introduction
|  | Recording
|  | Save
|  | Trigger display
|  | Open measuring file
|  | Select event
|  | Information
Introduction
| Gearshift viewer
A | Condition of the solenoid valves
B | Engine speed n1 Output speed n2
C | Engine acceleration a1 Output acceleration a2
D | Voltages Ul1, Ul2 and calculated pressures P1, P2 at integrator 1 and 2
| Starts recording of the measuring files
The program DIANA 5 ( DIagnosis and ANAlysis system ) is integrated in DIWAgnosis for recording the measuring files.
1 | Open files | 9 | Play back dataset
2 | Save measuring data | 10 | Start recording
3 | Exit DIANA 5 | 11 | Start/stop trigger function
4 | Show information | 12 | Show recording status
5 | ECU viewer | 13 | Show current front panel
6 | Select event | 14 | Switch front panels
7 | Stop dataseting | 15 | Show status
8 | Pause dataseting |  |
Recording Click "Start record" (10). DIANA 5 tries to communicate with the transmission control unit and loads an appropriate measuring template. This template contains different displays (virtual measuring instruments) that display the data of the transmission control unit (ECU). Depending on the measuring template, the displays may be distributed on several pages, the so-called front panels (13). While the recording is active, you can switch between the front panels using the function "Switch front panels" (14) via the numeric keys or via the options menu. As soon as data is received from the ECU, the status display (15) will burn green. The recording status is now "standby", meaning that data are now displayed but not yet recorded. Click again "Start record" (10). Recording is started and the status is now "record". You can pause and continue recording at any time. Save Click "Save measuring data" (2) to save the recording. The files are saved by default to the directory C:\Programm Files\DIWAgnosis 3.x\Records. Trigger display If the trigger display is active, the display may show "No Trg" in the recording status instead of "record". In this case, the recorder will only record if the measuring data meet the predefined trigger conditions. The recorder will then record all shifting and braking operations. You can deactivate the Trg function at any time by clicking the button "Activate/deactivate trigger function" (11); all signals will then be recorded. You can change the trigger criteria via the menu "Recorder", menu item "Trigger settings...". Open measuring file You can open a stored measuring file via menu "File", menu item "Open". You can continue the measurement or play the file back. Select event You can select a time event by clicking the button "Select event" or pressing the space bar. A window opens where you can name the event. Information You can view information about the transmission by clicking the button "Show information" or in the menu "Options", open the submenu "dataseting details...". Please refer to the online help to get further information.
© by Voith Turbo GmbH & Co. KG send remarks to markus.zwickel@voith.com (documentation department)