Operation
|  | Operator and control elements
|  | See also:
Operator and control elements Functions Keyboard The buttons for software configuration can be selected using the keys [ESC] – [F4]. Use the keys [A] – [L] to select the diagnostic functions in the main menu. Mouse Select functions directly by mouse-click. Move the mouse pointer over the buttons of the diagnostic functions to show their function. Control functions
| Exits DIWAgnosis.
| Opens the Online help.
| Starts communication to the control unit after communication failure.
| Loads function software and data record.
| Opens the Setup menu.
| Shows the currently set communication interface.
Diagnostic functions
| Read identification and connector pin assignment.
| Read or clear fault memory.
| Test gear selector switch.
| Test brake pedal.
| Test load transmitter.
| Reset adaptation
| Test solenoid valves and relays.
| Display active inputs.
| Gearshift viewer.
| Voltage and sensors.
| Select shift program
| Operational data acquisition and statistics.
Configuring the program setup Press function key [F4] or click the "SETUP" button. -> The Setup menu opens. Functions Note: You can select the functions using the keys or directly via mouse-click. [F3] Select user interface language. The functions "EXIT" and "HELP": The functions "EXIT" and "HELP" can be started from any menu.
| Click the EXIT button or press the [ESC] - key to return to the previous menu. When they are applied from the start menu, DIWAgnosis is exited.
| Click the HELP button or press the [F1] - key to activate the "DIWAgnosis Help" Online help function. The Online help works context-sensitive, i.e. it always displays the information required to assess, repair or operate the diagnostics element.
Please refer to the printed diagnostics manual for a detailed description of how to operate DIWAgnosis. See also:
|  | Aftersales service
© by Voith Turbo GmbH & Co. KG send remarks to markus.zwickel@voith.com (documentation department)