Analog temperature display
|  | Terminal connection diagram
|  | Test steps
Terminal connection diagram Test steps A temperature-dependent frequency signal applies at pin 22 on connector S2 or at corresponding pin (G) of temperature displaying unit. It can be checked using an oscilloscope or a multimeter with frequency measuring range.
© by Voith Turbo GmbH & Co. KG send remarks to markus.zwickel@voith.com (documentation department)