Setup
|  | Description
Description
| Setup
This dialog allows you to tailor the program to your requirements. Choose language for program dialogs. Colour selection for bars and LEDs. Selection of the directories and drives where the transmission function software and the data records are located and a directory for the log file which is created upon loading. A password is required to delete the operating data and to select shifting programs. The passwords are assigned by the VOITH customer service. The "baudrate" defines the speed with which PC and transmission control unit communicate. The higher this value, the faster communication will take place. A faster communication, however, may also be subject to interruptions. All serial ports are listed which exist in the control panel of the operating system i.e the permanently installed port (e.g. COM1) and also any retrofitted port e.g. using a PC card (e.g. COM3 or/and COM4). Please note that the settings will only become active if you have clicked the YES button before leaving the menu.
© by Voith Turbo GmbH & Co. KG send remarks to markus.zwickel@voith.com (documentation department)