Connector pin assignment on transmission side
|  | View of connector pins on transmission side
|  | General
|  | Configurable inputs (F)
|  | Inverted function (i)
|  | E200 connector pin assignment on transmission side
View of connector pins on transmission side General The above picture shows the pin assignment of the control unit on transmission side. The pin designation is indicated to the right of the pin number [red]. The function assigned to this particular pin is depicted next to it. Configurable inputs (F) Variable inputs allow their function to be selected via the data record, i.e. the data record specifies which function is activated at which pin. Inverted function (i) The control unit features inputs for switches that can be connected to ground (ELxx) and to +24 V (EHxx). For a switch to ground, the signal is usually active if a ground signal is on, and inactive if the input is open. This behaviour can be programmed in the data record of the control unit. This behaviour can be inverted via settings in the data record. E200 connector pin assignment on transmission side Apply menu item A "Read identification and pin assignment" to display a table of the current connector pin assignment of vehicle and transmission as specified in the record.
Signal | Pin | Explanation
-UB | 48 | Ground
52 | Ground
53 | Ground
LGIO2 | 24 | Load transmitter connection: PWM or voltage signal / USA: Oil level float switch Terminal A at J1587
LGIO3 | 5 | Load transmitter connection: PWM or ground / USA: Speed signal output
LGIO4 | 41 | Load transmitter connection: PWM or supply voltage Terminal B at J1587
EK | 19 | Output of input clutch solenoid
DK | 37 | Output of lockup clutch solenoid
SK | 18 | Output of overdrive clutch solenoid
PB | 2 | Output of pump brake solenoid
RBK | 21 | Output of reverse gear brake solenoid - small piston
( .3)WP | 3 | Output of converter pressure solenoid for DIWA.3 transmission
WR | 35 | Output of converter pressure control solenoid
RBG | 17 | Output of reverse gear brake solenoid - large piston
EKM | 15 | Input clutch measuring coil
DKM | 51 | Lockup clutch measuring coil
SKM | 33 | Overdrive clutch measuring coil
PBM | 14 | Pump brake measuring coil
RBKM | 13 | Measuring coil of reverse gear brake - small piston
( .3E)WP | 1 | Output of converter pressure solenoid for DIWA.3E transmission
TS+ | 8 | (+) input for temperature sensor
TS- | 44 | (-) input for temperature sensor
N1A | 11 | Input for inductive pickup to measure engine speed
N1B | 47 | Input for inductive pickup to measure engine speed
N2A | 29 | Input for inductive pickup to measure output speed
N2B | 10 | Input for inductive pickup to measure output speed
N3A | 46 | Input for inductive pickup to measure turbine speed
N3B | 28 | Input for inductive pickup to measure turbine speed
SENSE | 31 | Reference potential (ground) for measuring coils
© by Voith Turbo GmbH & Co. KG send remarks to markus.zwickel@voith.com (documentation department)