Pressure build-up
|  | Description
|  | See also:
Description Fault during pressure build-up while shifting. If this fault occurs, the precise cause of the malfunction must be localized by recording the shifting process
Fault type | Description
0001 | PB disk wear or incorrect engine torque settings during the 1→2 shift.
0002 | DK disk wear or incorrect engine torque settings during the 2→3 shift.
0004 | EK disk wear or incorrect engine torque settings during the 3→2 shift.
0008 | SK disk wear or incorrect engine torque settings during the 3→4 shift.
0010 | DK disk wear or incorrect engine torque settings during the 4→3 shift.
0020 | RBK disk wear or incorrect engine torque settings during RBK build-up.
See also:
|  | Aftersales service
© by Voith Turbo GmbH & Co. KG send remarks to markus.zwickel@voith.com (documentation department)