N2 output speed sensor
|  | Terminal connection diagram
|  | Test steps
|  | Important Note
Terminal connection diagram Test steps Open plug connection S1. Measure resistance between socket contacts 10 and 29 of cable 1. RTarget = 800-1400 Ω. If R = RTarget, continue with 4. Open S3. Check resistance between pin contacts E and F of cable harness or N2 contacts of measuring cable. RTarget = 800-1400 Ω. At transmission output: Remove cap over inductive pickup N2. Open S5. Measure resistance between pin contacts of inductive pickup N2. RTarget = 800-1400 Ω. Check resistance between contact 10 and vehicle ground at open plug connection S1. RTarget = ∞ Ω. Check resistance between contact 29 and vehicle ground. RTarget = ∞ Ω. Check resistance between contact E and ground at open plug connection S3. RTarget = ∞ Ω. Check resistance between contact F and ground. RTarget = ∞ Ω. Check resistance between each contact and ground at open plug connection S5. RTarget = ∞ Ω. Important Note If your check does not reveal any actual fault, please re-check the connecting cable to the sensor inside the transmission. In most cases, it is not the sensor that is faulted, but the cable!
© by Voith Turbo GmbH & Co. KG send remarks to markus.zwickel@voith.com (documentation department)