dNEUTR relay for power linkup
|  | Terminal connection diagram
|  | Test steps
|  | Notice: variable signal
Terminal connection diagram Test steps S2: Check resistance between corresponding contact and vehicle ground. RTarget = ∞ Ω. Notice: variable signal The assignment to a connection of the transmission control unit is accomplished in the data record and is vehicle-specific.
© by Voith Turbo GmbH & Co. KG send remarks to markus.zwickel@voith.com (documentation department)