Engine control unit - Bosch E-gas EMS 3.3 type B / G
|  | Terminal connection diagram
|  | Test steps
|  | See also:
Terminal connection diagram Test steps Open S2 plug connection (cable 2). Measure resistance between: contact 5 and corresponding contact at engine control unit (DKR), contact 41 and corresponding contact at engine control unit (DKV/PWM). R Target = 0 Ω. Check resistance of contacts 5 and 41 (cable 2) to vehicle ground. RTarget = ∞ Ω. See also:
|  | Engine control unit test - CAN SAE J1939 / IES
© by Voith Turbo GmbH & Co. KG send remarks to markus.zwickel@voith.com (documentation department)