Accelerator pedal - VDO stepless
|  | Terminal connection diagram
|  | Test steps
|  | See also:
Terminal connection diagram Test steps Open plug connection S2. Measure resistance between contacts in accordance with the following table. If all measurements yield R = RTarget, continue with point 3.
Position of accelerator pedal | Measurement between contact 5 (-LG) and: | RTarget [Ω] | Measurement between contact 5 (-LG) and: | RTarget [Ω]
0-load | 24 (+LG) | 800-1500 | 41 (LGM) | 178-333
Full load | 24 (+LG) | 800-1500 | 41 (LGM) | 622-1667
Open S3. Apply accelerator pedal in accordance with the following table and measure resistance between contacts.
Position of accelerator pedal | Measurement between contact 3 (-LG) and: | RTarget [Ω] | Measurement between contact 3 (-LG) and: | RTarget [Ω]
0-load | 1 (+LG) | 800-1500 | 2 (LGM) | 178-333
Full load | 1 (+LG) | 800-1500 | 2 (LGM) | 622-1667
S2: Check resistance of contacts 5, 24 and 41 to vehicle ground. RTarget = ∞ Ω. Open S3. Check resistance of contacts 1-3 to ground. RTarget = ∞ Ω. See also:
|  | Engine control unit test - CAN SAE J1939 / IES
© by Voith Turbo GmbH & Co. KG send remarks to markus.zwickel@voith.com (documentation department)