Important : 
To install Diwagnosis, it is important to have administrator rights on your computer.
The Voith Recorder COM port and language setting is done in the Diwagnosis Setup.



V E R S I O N    H I S T O R Y
------------------------------

DIWAGNOSIS 3.5.2
	- BlueCom Fix for newer laptops (e.g. Lenovo,...)

DIWAGNOSIS 3.5.1
	- *.bds files with index _00 to _99 were not created
	- Chinese language file fixed
	- COM Port handling simplified
	- DIANA Updated to 5.9.3

DIWAGNOSIS 3.5
	- Voith BlueCom K-Line Interface fully supported (Bluetooth and USB)
	- Windows Vista / Windows 7 compatible
	- Windows Vista / Windwos 7 : fsp, bds, d5m now in "My Documents\Diwagnosis\" folder
	- DIANA Recorder updated to version 5.9
	- Bugfix : Programming Protocol file without order number fixed

DIWAGNOSIS 3.4.5
	- Actuator fault priority setting for H5.1 possible
	- Automatic Bluetooth interface detection removed. Use Bluetooth checkbox in setup dialog.
	- Bugfix : Excel export, if data was loaded from a *.bds file
	- New programming method for all E200 ECU's with Bluetooth via ignition on/off

DIWAGNOSIS 3.4.4
	- Windows Vista compatible (use COM port >= 20 for Bluetooth)
	- Bds files can be directly opened by the Windows Explorer
	- Optimized Bluetooth communication (up to COM64 can be selected)
	- Toshiba Bluetooth Stack supported
	- More operational data is displayed, if *.bds file is loaded
	- Bugfix : No communication, if ECU was off at program start 


DIWAGNOSIS 3.4.3
	- Bugfix : Further polish and russian language problems fixed

DIWAGNOSIS 3.4.2
        - VOITH Bluetooth interface supported
	- Fsp files can be directly opened (valid file types : .fsp, .f00, .f01, f02, .f03)
	- Colors optimized in various views
	- ECU programming without ignition off (use Shift-F2, except for SW-Versions 18.22-18.25)
	- Last loaded software is automatically selected in the software selection list
	- Currently loaded software is marked with an asterisk
	- ECU software to load can be selected by a doubleclick
	- Flashing buttons in Load dialog
	- Show all entries of zuord.tab in selection list (Use Shift-F6)
	- Bugfix : Diwagnosis could crash with polish language
	- Bugfix : Programming protocols fixed

DIWAGNOSIS 3.4.1
        - Bugfix : Pin numbers of solenoid drawings corrected
	- Bugfix : Dataset without OEM name was not displayed in list for loading

DIWAgnosis 3.4
	- New languages : Russian and Romanian
	- Active shift program and transmission type displayed in identification data
	- Fault memory revised and extended
	- Export to Excel for operational data
	- Loading of dataset/software simplified
	- Keyboard navigation improved
	- Solenoid and actuator test for E200/H4
	- *.bds file only stored once per session
	- Older *.bds-files of same ECU will not be overwritten
	- E200/H4 bugfixes
	- Minor bugfixes
	- Actuator (not solenoid) test disabled for E200/H5.1 (hardware limitation)
	

DIWAgnosis 3.3
	- sorry, no detailed information about this version

DIWAgnosis 3.2 BUILD 20030305
	- majors changes in serial communication -> Speed up Flash (flash work ok at 57600 baud)
	- better control of threads used in the CFlashMemoryDlg and CFlashDataRecordDlg.
	- Flash: Wait for 3 seconds between the end of the software and the begin of the control unit.
	- add BUILD yyyymmdd at the title of the main dialog.
	- change DIWAgnosis 3.1 to DIWAgnosis 3.2 in the bitmaps and in the help files.
	- Add a button for Diana5 Recorder in the I menu.
	- change DIWAgnosis 3.1 to DIWAgnosis 3.2 in the installer and added the test for opperating system at the installation time.
	DIWAgnosis 3.2 will work only in Windows NT, 2000 and XP.
