TOEL oil temperature indicator
|  | Terminal connection diagram
|  | Test steps
|  | Notice: variable signal
Terminal connection diagram Test steps If the warning light for transmission oil is defective, replace light bulb. Open S2 plug connection. Check resistance between appropriate contact (of cable 2) and vehicle ground. With light bulb: RTarget = approx. 160 Ω. Without light bulb: RTarget = ∞ Ω. Measure resistance between appropriate contact and lead of the connecting cable to the transmission oil warning light. RTarget = 0 Ω. Measure resistance between – warning light cable and ground. RTarget = 0 Ω. Notice: variable signal The assignment to a connection of the transmission control unit is accomplished in the data record and is vehicle-specific.
© by Voith Turbo GmbH & Co. KG send remarks to markus.zwickel@voith.com (documentation department)