Engine control unit - CAN SAE J1939
|  | Terminal connection diagram
|  | Test steps
|  | See also:
Terminal connection diagram Test steps Open plug connections S2 and S3. Measure resistance between: contact 17 and contact A (CAN-H), contact 37 and contact B (CAN-L) contact 36 and contact C (CAN-M) . RTarget = 0 Ω. S2: Check resistance of contacts 17, 36 and 37 (cable 2) to vehicle ground. RTarget = ∞ Ω. See also:
|  | Engine control unit test - CAN SAE J1939 / IES
© by Voith Turbo GmbH & Co. KG send remarks to markus.zwickel@voith.com (documentation department)