CAN gear range selector E330 Inadmissible conditions at flexible output of CAN gear selector switch
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Connection of flexible output FLEXO-H1
|  | Connector pin assignment of CAN gear selector switch
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Test conditions of the event
|  | Final function check
|  | See also:
Description Inadmissible states have been detected while monitoring the flexible output. Effects on the driving operation The flexible output at the gear range selector can be non-functional. Possible causes Hardware fault of the gear range selector or the transmission control unit Connection of flexible output FLEXO-H1 Connector pin assignment of CAN gear selector switch
Pin | Name | Pin | Name | Pin | Name
1 | IGN | 6 | CAN-H | 11 | FLEXI-4
2 | -BATT | 7 | CAN-R | 12 | FLEXI-5
3 | CAN-L | 8 | FLEXI-1 | 13 | FLEXI-6
4 | CAN-L | 9 | FLEXI-2 | 14 | FLEXO-1H
5 | CAN-H | 10 | FLEXI-3 |  |
Place of action No description available. Instruction Clear fault memory and retest the gear range selector. Should the fault reoccur, please contact the VOITH customer service. Setting conditions of the event No description available. Test conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test the function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read out the fault memory. Check the transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions. See also:
|  | Aftersales service index
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)