Determination of desired gear Safety computer requests limp-home mode without reason
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Testing conditions of the event
|  | Final function check
Description The safety computer requests the limp-home mode alone without the main computer detecting a malfunction of the gear range selector. Effects on the driving operation The transmission first shifts to neutral. Driving can only be resumed if the limp-home switch is applied. Possible causes The safety computer alone does not receive valid information from the gear range selector. The main computer, however, still receives information from the gear range selector. This may be caused by an internal defect of the control unit. Place of action No description available. Instruction If problem occurs repeatedly, replace the control unit. Setting conditions of the event No description available. Testing conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read the fault memory Check transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions correctly.
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)