Transmission output speed sensor Undiagnosable fault
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Test conditions of the event
|  | See also:
Description Undiagnosible fault Effects on the driving operation No retarder operation Driving in reverse gear not possible or limited. No ANS-function Driving in 1st gear only. Higher gears at very high engine speed only (engine protection). If a substitute function is available, the fault may cause hard shifts and hard retarder activation. If the engine speed sensor is simultaneously defective, only limp-home mode is available. Possible causes No description available. Place of action Transmission output speed sensor Instruction No description available. Setting conditions of the event No description available. Test conditions of the event No description available. See also:
|  | Aftersales service index
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)