Vehicle-specific data Data set value AXLE_GEAR_RATIO_ faulty
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Testing conditions of the event
|  | Final function check
Description Data set value AXLE_GEAR_RATIO_ faulty. Effects on the driving operation Hard shifts incorrect blocking supervision Possible causes Dataset value AXLE_GEAR_RATIO_ lies outside the allowed range. Place of action No description available. Instruction Correct the dataset value AXLE_GEAR_RATIO_ or load a new dataset. Setting conditions of the event No description available. Testing conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read the fault memory Check transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions correctly.
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)