CAN brake signal source Brake pedal position faulty
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Testing conditions of the event
|  | Final function check
Description Brake pedal position faulty. Effects on the driving operation No ANS. No engaging of gears. No retarder function by brake pedal. Possible causes The value for the brake pedal position of CAN could not be determined due to a faulty value. (With SAE J1939 see EBC1(Electronic Brake Controller #1), 'brake pedal position' ). Place of action No description available. Instruction Check the CAN-message and contact the manufacturer of the transmitting control unit if necessary. (With SAE J1939 see EBC1(Electronic Brake Controller #1), 'brake pedal position' ). Setting conditions of the event No description available. Testing conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read the fault memory Check transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions correctly.
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)