Retarder oil temperature sensor Undiagnosable fault
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Location
|  | Instruction
|  | Setting conditions of the event
|  | Test conditions of the event
|  | See also:
Description Undiagnosible fault Effects on the driving operation Unable to detect temperature, possible consequences: The temperature-related deactivation of the retarder is restricted. Possible causes The cause could be a cable break or short-circuit to supply voltage. If the error 'Reference voltage too high' is also present, this indicates a short-circuit to supply voltage. If only one temperature sensor reports this fault, there is probably a cable break at this sensor. Location No description available. Instruction Check plug-in contacts, cabling and sensor. Setting conditions of the event No description available. Test conditions of the event No description available. See also:
|  | Aftersales service index
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)