TIM - Transmission Identification Module New TIM data available.
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Test conditions of the event
|  | Final function check
|  | See also:
Description New TIM data available. Effects on the driving operation The transmission control unit has recognized a new transmission. The configuration of the transmission control unit was adapted to the new transmission. Possible causes New software has been loaded into the transmission control unit. The transmission control unit was connected to a different transmission. Place of action Data in the TIM. Instruction Please verify whether the transmission configuration read out of the TIM matches the transmission actually connected! Setting conditions of the event No description available. Test conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test the function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read out the fault memory. Check the transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions. See also:
|  | Aftersales service index
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)