CAN gear range selector E330 The configuration memory (EEPROM) can not be addressed.
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Test conditions of the event
|  | Final function check
|  | See also:
Description The configuration memory (serial EEPROM) of the gear range selector can not be addressed. Effects on the driving operation The stored data of the gear range selector are not available. The gear range selector starts in the basic setting: * Driving is not possible or restricted. * The flexible inputs and flexible outputs could be non-functional. * Lighting of the gear range selector could remain dark. Possible causes Gear range selector defective. Place of action No description available. Instruction Clear the fault memory, park vehicle and restart. Check whether the fault is re-entered. If yes: Replace gear range selector. Setting conditions of the event No description available. Test conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test the function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read out the fault memory. Check the transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions. See also:
|  | Aftersales service index
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)