CAN-pushbutton switch E330 The configuration data of the gear range selector are faulty (checksum fault).
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Testing conditions of the event
|  | Final function check
Description The configuration data of the gear range selector are faulty (checksum fault). Effects on the driving operation Stored settings are not used. Gear range selector starts in the basic setting. Driving is not possible or restricted. The CAN bus is overloaded. Fabrication data, serial number etc. may not be correct! Flexible output and flexible inputs are non-functional. Possible causes Gear range selector defective. Place of action No description available. Instruction Replace gear range selector. Setting conditions of the event No description available. Testing conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read the fault memory Check transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions correctly.
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)