Engine load source PWM-signal (Bosch-EDC, MB-EMR, MB-FMR, VDO-EGas,...) Speed range in the data batch is faulty
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Testing conditions of the event
|  | Final function check
Description Speed range in dataset faulty. Effects on the driving operation Hard, in strong engines no shifts. Possible causes Data batch constant ENG_SPEED_RANGE_ faulty. Place of action No description available. Instruction Check/correct the elements of the dataset constant ENG_SPEED_RANGE_. If this is not possible, replace the dataset. Setting conditions of the event No description available. Testing conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read the fault memory Check transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions correctly.
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)