Coolant temperature sensor Undiagnosable fault
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Testing conditions of the event
Description Unknown fault. Effects on the driving operation No retarder operation. Possible causes The cause could be a cable break or short-circuit to supply voltage. If the fault 'Reference voltage too high' is also present, this indicates a short-circuit to supply voltage. If only one temperature sensor reports this fault, there is probably a cable break at this sensor. Place of action No description available. Instruction Check plug connections, cabling and sensor. Setting conditions of the event No description available. Testing conditions of the event No description available.
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)