TIM - Transmission Identification Module The TIM data in the memory of the transmission control unit are inconsistent.
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Testing conditions of the event
|  | Final function check
Description The TIM data in the memory of the transmission control unit are inconsistent. Effects on the driving operation The transmission control unit is performing a restart. Possible causes Internal fault of the control unit. Place of action No description available. Instruction Delete the fault from the fault memory. Restart the transmission control unit. If the fault reoccurs, check the connection between the transmission control unit and the TIM. If the fault occurs regularly, contact the Voith customer service. Setting conditions of the event No description available. Testing conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read the fault memory Check transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions correctly.
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)