CAN 1 - Hardware Invalid bit rate
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Testing conditions of the event
|  | Final function check
Description Invalid bit rate. Effects on the driving operation No CAN-communication via the CAN-controller 1 of the transmission control unit possible. Driving is not possible or restricted. Possible causes Software fault. The bit rate in the software of the transmission control unit does not correspond to the standard values 250 or 500. Place of action No description available. Instruction Please contact the VOITH customer service. Setting conditions of the event No description available. Testing conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read the fault memory Check transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions correctly.
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)