CAN Protocol SAE J1939 Timeout of message CCVS
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Testing conditions of the event
|  | Final function check
Description Timeout of the CAN receive message CCVS (CruiseControl / Vehicle Speed). Effects on the driving operation No ANS. Possible causes Controller for cruise control or connection to this controller is faulted. Place of action No description available. Instruction Check controller for cruise control (e.g. on-board computer, FFR, engine controller)and connection to this controller. Setting conditions of the event No description available. Testing conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read the fault memory Check transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions correctly.
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)