Shift program Short-circuit or low-resistance connection to ground at the digital input "SP selector"
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Location
|  | Instruction
|  | Setting conditions for the event
|  | Test conditions for the event
|  | Final function check
|  | See also:
Description Short-circuit or low-resistance connection to ground at the digital input "SP selector". Effects on the driving operation No changing of the shifting program possible. Possible causes Short-circuit or low-resistance connection of the input to ground. Location No description available. Instruction Check plug connections and cabling. Setting conditions for the event No description available. Test conditions for the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read the fault memory Check transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions correctly. See also:
|  | Troubleshooting a short-circuit to ground
|  | Aftersales service index
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)