Engine load signals via CAN CAN signal for idle switch position faulty
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Test conditions of the event
|  | Final function check
|  | See also:
Description CAN signal for idle switch position faulty Effects on the driving operation Hard shiftings. No ANS. Possible causes A CAN message required to determine the engine reference torque provides (a) faulty value(s). Using the SAE J1939 CAN protocol: CAN message 'EEC2' : CAN signal 'AP low idle switch' faulty. For information on the affected CAN message, please refer to the system description. Place of action No description available. Instruction Check the CAN message / CAN signal and correct if necessary. Setting conditions of the event No description available. Test conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test the function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read out the fault memory. Check the transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions. See also:
|  | Aftersales service index
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)