PB solenoid valve The operating coil is inadmissibly energised while switched off
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Connection of the solenoid valve
|  | Connector pin assignment of transmission control unit
|  | Pin assignment of transmission connector
|  | Internal cable harness
|  | Installation point of the solenoid valve
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Test conditions of the event
|  | Connector controllable solenoid valve
|  | Troubleshooting
|  | Final function check
|  | See also:
Description The operating coil is inadmissibly energised while switched off. Effects on the driving operation Driving is not possible. Automatic shift into neutral. Possible causes The output transistor autonomously generates voltage in the operating coil circuit due to an internal fault. Connection of the solenoid valve Connector pin assignment of transmission control unit
Pin | Stecker A | Stecker B | Stecker C | Stecker D
1 | SHIELD | EK | FLEXI-1 | -BATT
2 | TIM+ | DK | --- | IGN
3 | TIM- | SK | FLEXI-3 | FLEXI-11
4 | N1+ | RBK | FLEXI-4 | K-LINE
5 | N1- | TB | FLEXI-5 | CAN1-H
6 | N2+ | --- | FLEXI-6 | CAN1-H
7 | N2- | RBG | FLEXI-7 | CAN-SHLD
8 | N3+ | PB | FLEXI-8 | CAN1-L
9 | N3- | WR | FLEXI-9 | CAN1-L
10 | --- | WP | FLEXI-10 | CAN2-H
11 | --- | --- | FLEXO-2H | CAN2-H
12 | EKM | FLEXI-12 | FLEXO-4H | CAN2-L
13 | DKM | S-GND | FLEXO-3H | CAN2-L
14 | SKM | OIL-LVL | FLEXO-5L | CAN1-R
15 | PBM | T-SUMP | --- | ---
16 | TBM | --- | --- | FLEXO-1L
17 | RBKM | T-CONV | --- | CAN2-R
18 | MVM-GND | MV-GND | --- | +BATT
Pin assignment of transmission connector
Pin | Name | Pin | Name | Pin | Name
1 | S-GND | 14 | RBK | 27 | EKM
2 | MV-GND | 15 | RBG | 28 | PBM
3 | MV-GND | 16 | TB | 29 | RBKM
4 | --- | 17 | WR | 30 | TBM
5 | T-CONV | 18 | --- | 31 | MVM-GND
6 | T-SUMP | 19 | --- | 32 | N1+
7 | OIL-LVL | 20 | --- | 33 | N1-
8 | P-DIFF | 21 | TIM- | 34 | N2+
9 | SK | 22 | TIM+ | 35 | N2-
10 | DK | 23 | --- | 36 | N3+
11 | EK | 24 | SHIELD | 37 | N3-
12 | PB | 25 | SKM |  |
13 | WP | 26 | DKM |  |
Internal cable harness Installation point of the solenoid valve Place of action Transmission control unit Instruction Replace transmission control unit. Setting conditions of the event No description available. Test conditions of the event No description available. Connector controllable solenoid valve
Pin assignment for solenoid valve 4 = operating coil: connection to supply 2 = operating coil: connection to ground 1 = measuring coil: connection to supply 3 = measuring coil: connection to ground |  |
Troubleshooting Replace the transmission control unit. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test the function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read out the fault memory. Check the transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions. See also:
|  | Aftersales service index
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)