Determination of desired gear Dataset value FLEXI_FRCD_NEUTRAL_SETTING_ is faulty
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Testing conditions of the event
|  | Final function check
Description Dataset value FLEXI_FRCD_NEUTRAL_SETTING_ is faulty Effects on the driving operation The forced-neutral function is inactive. The forced-neutral function shifts the transmission into neutral if a signal applies at the forced-neutral input of the transmission control unit. Possible causes The dataset is faulty Place of action No description available. Instruction Request new dataset from Voith. Load correct dataset. Setting conditions of the event No description available. Testing conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read the fault memory Check transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions correctly.
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)