Transmission output speed sensor Undiagnosable fault
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Testing conditions of the event
Description Unknown fault. Effects on the driving operation No retarder operation. No switching into reverse gear. No ANS-function. Only change gears to protect the engine against under or over-speed. For substitute functions, possibly hard shifts and hard retarder activation. If the engine transmission output speed sensor is simultaneously defective, only limp-home mode available. Main pressure to maximum. Reduction of the engine torque to protect the transmission. Possible causes No description available. Place of action Transmission output speed sensor Instruction No description available. Setting conditions of the event No description available. Testing conditions of the event No description available.
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)