TIM - Transmission Identification Module New TIM data available.
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Testing conditions of the event
|  | Final function check
Description New TIM data available. Effects on the driving operation The transmission control unit has recognized a new transmission. The configuration of the transmission control unit is adapted to the new transmission. Possible causes New software has been loaded into the transmission control unit. The transmission control unit was connected to a different transmission. Place of action No description available. Instruction Please verify whether the transmission configuration read out of the TIM matches the transmission actually connected! Setting conditions of the event No description available. Testing conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read the fault memory Check transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions correctly.
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)