Transmission output speed sensor Fault while measuring the sensor voltage
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Test conditions of the event
|  | Final function check
|  | See also:
Description Fault while measuring the sensor voltage Effects on the driving operation No retarder operation Driving in reverse gear not possible or limited. No ANS-function Driving in 1st gear only. Higher gears at very high engine speed only (engine protection). If a substitute function is available, the fault may cause hard shifts and hard retarder activation. If the engine speed sensor is simultaneously defective, only limp-home mode is available. Possible causes Error while reading the sensor voltages U(nA) or U(nB). The fault is probably located inside the control unit. Place of action Transmission control unit Instruction Replace transmission control unit. Setting conditions of the event No description available. Test conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test the function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read out the fault memory. Check the transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions. See also:
|  | Aftersales service index
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)